# The Project Gutenberg eBook, Advanced Toy Making for Schools, by David M. Mitchell

    This eBook is for the use of anyone anywhere at no cost and with
    almost no restrictions whatsoever.  You may copy it, give it away or
    re-use it under the terms of the Project Gutenberg License included
    with this eBook or online at www.gutenberg.org

Title: Advanced Toy Making for Schools

Author: David M. Mitchell

Release Date: July 22, 2011 [eBook #36815]

Language: English

Character set encoding: ISO-8859-1

***START OF THE PROJECT GUTENBERG EBOOK ADVANCED TOY MAKING FOR SCHOOLS***

#### E-text prepared by Chris Curnow
and the Online Distributed Proofreading Team
(http://www.pgdp.net)
from page images generously made available by
Internet Archive
(http://www.archive.org)

Note: | Images of the original pages are available through Internet Archive. See http://www.archive.org/details/advancedtoymakin00mitc

# ADVANCED TOY MAKING
FOR SCHOOLS

#### BY

## David M. Mitchell

#### Instructor Manual Arts
Willson Junior High School, Cleveland, Ohio

### The Manual Arts Press
Peoria, Illinois

Copyright 1922
David M. Mitchell
12 B 22
Printed in United States of America

[Pg 3]

## PREFACE

oys are today regarded as educational factors in the life of boys and girls. New toys come into demand at frequent intervals in the growth and mental development of the child. On account of the unfailing interest on the part of the pupils in toys and because of the unlimited educational possibilities contained in toy making, this work is rightfully taking an increasingly important place in the manual arts program in the schools.

This book is the outgrowth of toy-making problems given to junior-high and high-school pupils. The author claims no originality for some of the toys. However, most of them have been originated or improved upon in the author's classes.

While it is entirely satisfactory to have any of the toys mentioned in this book made as individual projects, they are here offered as suitable group projects or production projects, and it is hoped that the suggested form of shop organization for production work as treated in Part I is flexible enough so that the plan can be applied to most any shop conditions.

The drawings of toys in Part II will suggest a variety of articles which may be used in carrying out the production work.

Of course, the success of organizing and conducting classes for this kind of work depends largely upon the instructor. He must know definitely what he is trying to get done. He must adopt and pursue such methods of dealing with both the members of the class and the material as will contribute directly towards the desired end.

Toy making carried on by the so-called productive plan, if handled properly, will bring out many of the essentials of an organization typical of the commercial industries. Together with its educational possibilities and its power to attract the attention of those engaged in this activity, toy making will rightfully take its place alongside other important subjects offered in a complete industrial arts course.

The author wishes to acknowledge his[Pg 4] indebtedness to William E. Roberts, supervisor of manual training, Cleveland Public Schools, for valuable suggestions and inspiration; to Joseph A. Shelley, Jersey City, N. J., for suggestions on finishing kiddie car wheels; to the Eclipse Air Brush Company, Newark, N. J., for valuable information and photographs of air brush equipment; and to the American Wood Working Machinery Co., for the use of the illustrations showing the operation of the turning lathe, universal saw, and other woodworking machines.

Cleveland, Ohio, 1921.

D. M. Mitchell

[Pg 5]

## CONTENTS

### PART I
Operations in Toy Making

Chapter I. Productive Work | 11
1. Suggested plan for shop organization. 2. Grouping of students. 3. The time clerk and tool-room clerk. 4. Recording attendance. 5. Time cards. 6. Using time card. 7. Grading students. 8. Preliminary discussion and preparation for shopwork. 9. Bazaars, toy sales, etc.
Chapter II. Coloring Toys | 21
10. Sanitation emphasized. 11. Preparation of surfaces. 12. Application of water colors. 13. Analine water stains. 14. Formulas for analine water stains. 15. Oil stains. 16. Shellacking. 17. Varnishing. 18. Points on Varnishing. 19. Colored varnish. 20. Another suggestion for finishing. 21. Use of paint. 22. Ingredients of good paint. 23. Application of paint. 24. Preparation of surface. 25. Tinting materials. 26. Mixing paints. 27. Paint formulas. 28. Formulas for making tinted paint. 29. Enameling. 30. The dipping method. 31. Polishing by tumbling. 32. Care of brushes. 33. Paint application by means of compressed air. 34. Uses of pneumatic sprayers. 35. Construction of pneumatic painting outfit. 36. Special attachments for different surfaces. 37. Cleaning pneumatic machines. 38. Directions for cleaning machine. 39. Directions for operating pneumatic equipment. 40. Preparing colors.
Chapter III. Common Woods Used in Toy Making | 42
41. Economy in selecting material. 42. Qualities of different woods used.
Chapter IV. Use of Jigs and Fixtures | 43
43. Value of jigs and fixtures. 44. Cutting small wheels. 45. Turning wheels. 46. Use of wheel cutter. 47. Use of coping saw. 48. Cutting sharp corners. 49. Removing the saw-blade from frame. 50. Making heavy wheels. 51. Designs for wheels. 52. Cutting wheels on band-saw. 53. Boring holes in wheels.
Chapter V. Operation of Woodworking Machines | 54
54. Importance of machine operations. 55. Operating the lathe. 56. Face plate turning. 57. The universal saw. 58. The hand jointer. 59. The sander.

[Pg 6]

### PART II
Drawings for Toys

|  | PAGE
Plate | 1. Fox and Geese Game | 64
" | 2. Ring Toss | 65
" | 3. Baby's Cart | 66
" | 4. Hay Cart | 67
" | 5. Horse Head | 68
" | 6. Horse on Wheels | 69
" | 7. Kido Kar Trailer | 70
" | 8. Auto Roadster | 71
" | 9. Auto Racer | 72
" | 10. Passenger Car | 73
" | 11. Milk Wagon | 74
" | 12. Table for Doll House | 75
" | 13. Chair and Rocker | 76
" | 14. Buffet | 77
" | 15. Toy Wheel-Barrow | 78
" | 16. Horse Barrow | 79
" | 17. Doll's Carriage | 80
" | 18. Noah's Ark | 81
" | 19. "Bean Bag" Game Board | 82
" | 20. Child's Swing No. 1 | 83
" | 21. Child's Swing No. 2 | 84
" | 22. Doll's Bed, No. 1 | 85
" | 23. Doll's Bed, No. 2 | 86
" | 24. Adjustable Stilts | 87
" | 25. Scooter | 88
" | 26. Steering Coaster | 89
" | 27. Kido Kar | 90
" | 28. Kid Kar Junior | 91
" | 29. Pony Kar | 92
" | 30. Duplex Speedster | 93
" | 31. Rock-a-Doodle | 94
" | 32. Sled | 95
" | 33. "Sturdy Flyer" Sled | 96
" | 34. Ducky Loo | 97
" | 35. Duck Rocker | 98
" | 36. Jitney | 99
" | 37. Junior Roadster | 100
" | 38. Details of Junior Roadster | 101
" | 39. Senior Coaster | 102
" | 40. Details of Senior Coaster | 103
" | 41. Auto-Kar | 104
" | 42. Choo-Choo-Kar | 105
" | 43. Teeter-Totter | 106
" | 44. Teeter Rocker | 107
" | 45. Checker Board | 108
" | 46. Child's Costumer | 109
" | 47. Baby's Chair | 110
" | 48. Children's Sand Box | 111
" | 49. Sand Box No. 2 | 112
" | 50. Doll's House No. 1 | 113
" | 51. Doll's House No. 2 | 114
" | 52. Doll's House No. 2 | 115
" | 53. Dumb Bell & Indian Club | 116
" | 54. Bats | 117

[Pg 7]

## SUGGESTIONS TO TEACHERS

Where the work is to be done on the so-called productive basis, it is of utmost importance that, before starting, the classes should be so organized as to allow the work to be carried on in the most efficient, progressive manner. The form of shop organization suggested in this book is recommended. However, the instructor may, particularly if he has had good practical shop experience, employ other methods of organization that are just as good and possibly even better for his particular class and the conditions under which he has to work.

It is also of great importance that the instructor should acquaint himself with the processes involved in the making of each toy before allowing the class to begin it. This may be accomplished by the making of a sample of the contemplated project, carefully analyzing its different parts and arranging the operations in a logical sequence. This phase of the work may be done during class discussions and demonstrations at which time the different jigs and fixtures needed for progressive production may also be developed.

The different methods of coloring toys have been suggested with the hope that the student will gain a realization of the importance of finishing, from both the artistic and the practical point of view. The application of paint by means of compressed air is the latest development in the coloring of toys, and an equipment in the school shop illustrating the principles of compressed air as applied to productive finishing of toys, is a step forward in making school shops function as they should.

The working drawings in this book should serve as suggestions. They have been so constructed as to be free from unnecessary technicalities, and to leave as much opportunity as possible for the exercise and development of the student's judgment.

It will be found that toy making offers itself readily to the desired co-operation and correlation with other departments in the school. For instance, the art department may aid with the designing and color scheme to be used on toys; the general metal shop may help in the making of necessary metal parts: the mechanical [Pg 8] drawing department can co-operate in the making of working drawings; the mathematics department can figure the costs of production, etc., etc.

It is hoped that the purpose of this book is not merely to set forth a few plans and drawings for the construction of toys, but to give the work the broadest possible application; creating a constructive influence on the minds of the students, in which case it will also act as a means of bringing into closer relationship their life outside of school with the work in school.[Pg 9]

[Pg 10]

Toy Making on a Productive Basis Employing Factory Methods

[Pg 11]

# PART I

# Operations in Toy Making

## CHAPTER I

## Productive Work

1. Suggested Plan for Shop Organization.—While it is entirely satisfactory to have any of the toys mentioned in this book made as individual projects, they are here offered as suitable group projects or production projects. Production work may be defined as work done by a class to turn out a number of similar projects that have a marketable value, with the aid of jigs, fixtures, and other means of duplication, illustrating the industrial or practical application to the tasks in hand, Figs. 1, 2, and 3. This does not mean, however, that the school shops be transformed into a factory in the full sense of the word. It should differ from a factory in that the education of the student is the major part of the product, while in the factory production is the foremost aim.

In doing work by the productive plan two important problems will present themselves at the outset; first, the time element; and second, industrial or practical application to the tasks in hand.

A brief explanation of the plan of organization in one of the author's classes will attempt to show how nearly these problems can be solved.

Fig. 1. Material for toys, prepared on a large scale

2. Grouping of Students.—Classes are divided into groups of between four and six boys, with a boy foreman appointed at the head of each group. The foreman is held responsible for the work turned out by his boys. He is to see that they understand just what is to be done and how it is to be done. All the group foremen are directly responsible to the general foreman who in turn is responsible to the instructor. The [Pg 12]general foreman is to act as an inspector of finished work after it has received the group foreman's O.K. He is also held responsible for the condition of the shop during his class hour. This includes looking after all material, the manner in which stock is put away after class, and adherence to all shop rules that have been adopted to help in the efficiency of shop procedure.

[Pg 13]

Fig. 2. A large order of toys partly constructed

3. The Time Clerk and Tool-Room Clerk.—A "Time Clerk" is appointed to take charge of the time cards. He is also held responsible for all the clerical work that is to be done in the shop.

A Tool-Room Clerk is appointed to take charge of the shop tool room. He is to keep check of all tools given out and taken in. His spare time should be devoted to the care of tools.

If possible, each boy in the class should be given an opportunity to act in each capacity that has been created, so that he may get the most varied experience in shop procedure. This will necessitate the changing of boys from one[Pg 14] group to another; the changing of foremen, clerks, etc., at intervals which will of course be governed by the size of the class and the number of hours devoted to the work.

Fig. 3. Milk wagons completed by the production method
Fig. 4. The time-card rack.

4. Recording Attendance.—Boys, upon entering the shop, register their presence at the Time-Card Rack, Fig. 4. This is done by turning the time card shown in Fig. 5, so that the back side, which has the word present printed at top, is exposed. The time clerk then inspects the cards and notes those that have not been turned, and records the absences. He then fills in the date and passes the cards out to the boys in the shop. Toward the latter part of the period, a few minutes time is given the boys to fill in the necessary data on the time card.[Pg 15]

The time cards are then collected by the time clerk and put into a box where the time cards of all the classes are kept. In the meantime the time clerk puts back into the time rack the cards of the incoming class. This duty is performed by the time clerks of all the classes, thereby necessitating the use of only one time card rack.

5. Time Cards.—Referring to the time card mentioned in Fig. 5 it will be seen that the workman's shop number is filled in at the top. Then under the heading of "Woodworking Department" are two horizontal rows of items which need very little explanation. Following are three columns headed "Operation," "Assignment," and "Time." Below the word "Operation" are set down the various operations undertaken in the woodworking department, with several vacant spaces provided where other and special operations can be filled in. It will also be noticed that "Operations" are divided into two kinds, machine work and bench work. The instructor's glance at the time card will tell him at once what phase of the work the boy has been employed in and will help him in apportioning the work so that the boy is offered a varied experience.[Pg 16]

6. Using Time Card.—For shops that are not equipped with the kind of machines marked on the illustrated card, it would be well to omit the names of machines in the "operation" column. The instructor may then fill in the operation whatever it may be.

Under the heading "Assignment" and against the operation which is to be undertaken by the student, the instructor writes in the name of the part to be made. This is the student's assignment and it should be read by him at the time he records his presence at the time-card rack upon entering the shop.

In making assignments, the instructor may find it rather difficult to keep up with large classes of boys. This difficulty may be overcome by making an assignment to an entire group instead of to each boy. For example, in a class of twenty-five that would probably be divided into five groups, the instructor may make the assignment to the foreman of each group and each foreman in turn can inform the boys of his group as to the nature of the assignment. The boys can then enter the assignment on their time cards at the end of the period when the time spent on the job at hand is also recorded.

Fig. 5. Time card

The student's shop number, name, and grade should be filled in by the time clerk who can get out a number of cards for each student in advance and these are kept ready for use by the instructor. The instructor can then mark the project and the job number together with the student's assignment. At the same time he estimates the journeyman's time and rate and enters them in the space provided.

The time card in Fig. 5, is 3½ inches by 9 inches, made of three-ply bristol board. All worker's cards are printed on white colored bristol while those of the foremen are of blue colored bristol. This plan is for the instructor's convenience to be able to pick out the foremen's time cards at a glance.

In the triple column under the heading "TIME" is provided room for the date and spaces in which the student can write the time in minutes spent on the various operations on that date. The triple columns on each side of the card allow of the cards being used for six days. If a job lasts longer than six days another card should be used marking them No. 1 and[Pg 17] No. 2, respectively, in the space marked "Card No." Both cards should be fastened and kept together.

Effort should always be made to have all the assignments short (less than six days) so that the student's record may be computed at the end of each week by the time clerk.

7. Grading Students.—The next four spaces contain in condensed form, the information itemized in other parts of the card. This, together with other information set down by the instructor, is the vital material sought for.

The item A "Journeyman's Time" is very easily recorded by the instructor. It is arrived at in the same way as in making out the estimate for any piece of work and can be recorded almost at once. The main purpose here is to set for the student a standard of time on which to work.

The item B is the rate in points per hour, based on the journeyman's time.

The item C is the total of the student's time added together from the various spaces under "Time."

Item D "Quality Decimal" is the quality of the student's job expressed in the form of a[Pg 18] decimal, with 100% as the maximum. This mark should be filled in by the instructor when the student completes his job.

The next item, the number of points the student earns is found by the formula Points = (A×B)D

Points earned per hour = | (A×B)D C

Fig. 6. Monthly accomplishment sheet

For example, a student receives an assignment to cut to thickness, width, and length, sixty chair legs. The size of the legs he is to get from the job blueprint. He spends 60 minutes a day, for three days, making a total of 180 minutes or 3 hours. The time it would take a journeyman to do the same job is estimated at 2 hours. The rate adopted is at 80 points per hour; the journeyman therefore earns A×B = 2×80 = 160 Points. The quality of the student's job is graded by the instructor as 75%. The number of points the student earns is found by the formula Points = (A×B)D = (2×80).75 = 120 Points. To find the number of points the student earns per hour, divide 120 points by the number of hours it took the student to complete the job, which equals 120 ÷ 3 = 40, the number of points the student earns per hour. However, if the student would be graded 100%, he would earn the same number of points as the journeyman. But of course, he would have done it in three hours where the journeyman has earned[Pg 19] the same number of points in two hours. It will readily be seen that this scheme offers the student an everlasting incentive to equal the journeyman's record.

Having obtained the points on the time card or assignment card as it may be called, these are then transferred to a monthly accomplishment sheet as shown in Fig. 6, which is provided for all the students in all classes.

The total number of points for each boy, group, and class can then be easily obtained. These totals can be put up in poster form and hung on the shop's bulletin board, showing the standing of each boy, group, and class. It is surprising the amount of interest and competition that can be aroused; everyone working for the highest honors, unconsciously, with a competitive spirit that will bring out considerable thought and effort to the matter of handling material for maximum production.

8. Preliminary Discussion and Preparation for Shopwork.—Of course, no time card or assignment-record scheme can hope entirely to eliminate the necessary preliminary discussions and preparation. The author has found it of material help to meet the foremen of all the classes at hours other than their regular class hour and discuss such topics as "Securing Cooperation," "Instructing Workers," "Maintaining Cleanliness and Order," "Records and Reports," "Inspecting Work," "Routing Material Thru Shop," "Care of Stock," etc.

Details regarding construction and assembling should be worked out by the instructor beforehand, and also developed with the class as the work progresses. Care should be taken that plans are carefully made regarding the storage of stock and unfinished parts.

The old saying, "An ounce of prevention is worth a pound of cure," is an old one, but a good one.

9. Bazaars, Toy Sales, Etc.—The plan of selling toys, that are made in the school shop, to the boys and girls of the school is a plausible one. It can very easily be accomplished in the form of bazaars, exhibitions, or school toy sales.

The writer has had a number of samples of different toys made and put on exhibition, and orders taken, requiring a deposit on each order. These were then turned in to the shop department and the toys made on the productive plan.[Pg 20]

The boys in the shop would receive school checks, Fig. 7, for the total number of points that they earned for the semester. These checks could then be used by them towards the purchasing of any of the toys that were put on sale; a certain number of points required for the purchase of different toys.

Fig. 7. Credit check, based on number of points carved

This plan was made possible by adding on to the number of orders received an additional number equal to the number of boys in the shop. For example, twenty-four orders for toy milk wagons were received by a class of twenty-four boys. Then instead of making twenty-four toy milk wagons we doubled the number and made forty-eight of them. The price that was figured on for the twenty-four orders would more than cover the cost of material for the other twenty-four articles that the boys would be able to buy with their earned checks.

[Pg 21]

## CHAPTER II

## Coloring Toys

10. Sanitation Emphasized.—All application of color to toys should carry with it a realization that toys are meant primarily for children and that all paints should therefore be free from poisonous compounds.

All paints used should be of good quality so that it will not come off easily to discolor the hands or tongues of children who cannot resist the temptation of sticking everything possible into their mouths.

11. Preparation of Surfaces.—Wooden toys may be finished quite bright and in various colors.

Before applying the color it is absolutely necessary that every part of the toy has been thoroly sanded. Where sanding is done by machine, care should be taken not to sand the wood too much. Many difficulties may arise from too much as well as from too little sanding. In hand sanding, the use of a block 2½" × 3½", to which is glued a piece of cork, is recommended.

12. Application of Water Colors.—Toys may be colored by the use of different materials and by various methods. Kalsomine colors, opaque water colors, variously known as show card colors, liquid tempera, and letterine,—all come under the heading of water colors. All but the kalsomine may be obtained in small jars and ready for use. Kalsomine colors come in powder form in various colors and may easily be prepared by mixing with water and a little glue to bind the parts together. They are much cheaper than the ordinary forms of transparent and opaque water colors. They may be applied with the ordinary water color brushes.

After a coat of water color has been applied to the toy, it may be necessary to remove the rough parts with very fine sand paper. Care should be taken not to "cut thru" when sanding.

To preserve and protect the water color on the toy a coat of white shellac may be applied. If a more durable finish is desired a coat of good clear varnish over the shellac will serve the purpose.[Pg 22]

13. Analine Water Stains.—For general finishing of toys analine water stains will produce excellent results. They are known for their ability to penetrate the wood deeply and the ease with which any shade can be produced. Water stain raises the grain of the wood more than any other. This makes it necessary to sandpaper down the raised grain until smooth and then proceed with the shellacking and varnishing until the desired results are obtained.

In preparing analine water stains, only analines that are soluble in water are used. Place an ounce of the analine to a quart of hot or boiling water, pouring the water over the dye-stuff and stirring meanwhile with a wooden paddle or stick. Soft water is the best. In about an hour the dye may be filtered thru a piece of fine woven cloth. As metal is apt to discolor the dye, it is better to use a glass container. If the prepared solution is too strong it may be diluted in more water. Use hot water for diluting the stain.

The work with water stain must be done quickly in order to obtain a uniform coloring on the surface. Water stains are used a great deal where the dipping process is employed in the finishing of toys. A hot dipping stain is preferable to a cold dipping stain, first, because it penetrates more readily and second, because it dries quicker.

14. Formulas for Analine Water Stains.—(Stock Solutions).

Red: Rose benzol five parts, water ten parts.

Rose Red: Dissolve 3 oz. Rose Bengal in 5 pints of water.

Blue: (a) Dissolve 1 oz. of the best indigo carmine in 8 oz. of water. (b) Prussian blue dissolved in water.

Dark Blue: Dissolve 3 oz. Bengal blue in 3½ pints of boiling water, and stir and filter the fluid in ten minutes time.

Green: Mix Prussian blue and raw sienna in such proportions as will give the desired color. Mix in water.

Brown: Dissolve 3 oz. of Bismark brown in ½ gal. of water.

Yellow: Auramine 4 parts, sulphate of soda 10 parts, mixed in water.

Black: Nigrosine black, four ounces, dissolved in one gallon of boiling water.

When wanted for use, these analines may be[Pg 23] diluted with water. The rule is, an ounce of analine to the gallon of water to form a working stain. Or to a pint of the stock solution, as it is called, you may add three pints of water.

15. Oil Stains.—It will be found that quicker work can be done with oil stain than with water colors. For that reason, oil stains are also used a great deal as a dipping stain. In preparing oil stains, the best mineral or earth pigments to dissolve with turpentine are Van Dyke brown, chrome green, burnt and raw sienna, and lamp black.

16. Shellacking.—There are two kinds of shellac, orange and white. The white shellac is orange shellac that has been bleached. The purpose of shellac as commonly understood is to give a quick coat over the stain. The thin coat formed serves as a protector for the stain and also as an undercoater for the following coat of varnish. In this way at least one coat of varnish is eliminated and a great deal of time saved because the shellac dries within a few minutes. To thin shellac use denatured alcohol.

On cheaper toys a coat of shellac only may be used as a covering for the color stain. If orange shellac is used it will be found that it effects the color of the stain used. White shellac also produces a slight change in color and for this reason many working with toys will use a good clear varnish instead.

17. Varnishing.—Two or three coats of varnish will produce a very durable finish. The first coat of varnish ought not be quite as heavy as the succeeding coats. If the varnish is of extra heavy body it should be reduced slightly for the first coat. The best varnish reducer is thin varnish. To prepare this reducer, take one part varnish (the same varnish to be reduced), and two parts of turpentine. Shake these together well and let stand twenty-four hours before using. This will reduce the consistency of the varnish without tearing down the body as pure turpentine would. The first coat of varnish should be allowed to dry thoroly before the second coat is applied.

Oil varnishes made from good hard gums, pure linseed oil, and turpentine, are the most valuable. In using turpentine to thin varnish care should be taken that adulterated turpentine is not used. To play the game safe it is advisable to use a little benzine, for it will not injure the varnish, but will evaporate entirely,[Pg 24] and not flatten the varnish as turpentine does.

18. Points on Varnishing.—(1) The less varnish is worked under the brush the better its luster. (2) Use clean brush and pot, and clean varnish. See that the surface is clean before beginning to varnish. (3) Allow a coat of varnish plenty of time for drying until it becomes hard.

19. Colored Varnish.—Colored varnish is that in which a proportion of varnish is added to the pigment and thinned. The base is usually an earth color such as ochre, sienna, venitian red, Van Dyke brown, umber, lamp black, etc.

With this the work can be done in one coat. This method of finishing is usually employed on the cheaper class of toys where it isn't advisable to apply an expensive finish.

20. Another Suggestion for Finishing.—Tint a gallon of benzine or gasoline with chrome green, chrome yellow, and vermilion, ground in Japan until the desired shade is obtained. This formulae is especially good for dipping purposes.

21. Use of Paint.—Although paint can be bought ready prepared and in any color, as has been stated, it is advisable to have the students mix their own colors and choose their own color scheme.

22. Ingredients of good Paint.—The best paints are usually made by mixing together white lead, linseed oil, pigment of the desired color (colors ground in oil), and a drier.

While white lead is sufficient as the pigment for white paint, a better result is obtained by mixing zinc oxide with the white lead. These two substances have the convenient property of balancing each other's disadvantages. For instance, zinc oxide has a tendency to crack and to peal, which is overcome by the tougher coating formed by the white lead. Again, when white lead is exposed to light and weathering, it becomes chalky, which fault is remedied by the property possessed by zinc oxide, of remaining hard.

The linseed oil used is obtained from flaxseed by pressing the thoroly ground seed. About twenty-three gallons of oil can be obtained from one bushel of the seed. By boiling the oil with lead oxide or manganese oxide it can take more oxygen from the air, and thereby its drying powers are increased.

Driers are substances that absorb oxygen[Pg 25] from the air and give part of it to the oil. The raw linseed oil absorbs the oxygen from the air very slowly, but the addition of turpentine is a great aid in overcoming this defect.

To insure the best results in painting, one must first consider the kind and condition of the surface to be painted, and to what use the toy will be put; then decide on the proper composition and consistency of the paint.

23. Application of Paint.—In applying the paint to the toy the first coat should be thinned. This will act as a primer or undercoat for the succeeding coats of paint. Care should be taken that plenty of time is allowed between coats for the paint to dry thoroly. Three coats of paint will produce a good finish.

24. Preparation of surface.—All woodwork must be sanded and thoroly dry before any paint is applied. Care should be taken to see that all knots and sappy streaks shall be covered with a coat of orange shellac. Then apply the first coat.

After the priming coat of paint is thoroly dry, putty up all knot holes, dents, cracks, and other defects in the surface with a pure linseed oil putty composed of equal parts of white lead and whiting. When putty is dry, proceed with the other coats.

25. Tinting Materials.—Formulas for making tints are to be followed only in a general way. Make some allowance for slight variations in the strength and tone of different makes of colors. Chromes and ochres vary noticeably. Weigh out your color and add it gradually, not all at once, noting the effect as you go. When you reach the desired shade, stop, regardless of what the formula calls for. Turpentine and dark driers will slightly alter shades. Make allowance for this.

26. Mixing Paints.—Faulty mixing, even with the best of materials, is not likely to make durable paint. The important thing is to give the lead and oil a chance to incorporate themselves in that close union which they always make if allowed to do so. The following directions give best results. The order is important.

(1) Break up the white lead with a paddle, using only enough oil to bring it to the consistency of colors in oil.

(2) Add your colors for tinting. Coloring matter added after the paint has been thinned is likely to break up in lumps which leave streaks[Pg 26] when brushed out.

(3) Put in drier.

(4) Add remainder of oil, stirring well.

(5) Last of all, put in turpentine.

Thinners help only the flow of the paint never the quality.

To strain paint thru cheese cloth before using will be a safeguard against lumpy colors and streakiness. Paint also spreads further if strained.

27. Paint Formulas.—As most toys are exposed to the weather a great deal, the following formulas are recommended. These take no account of tinting materials.

(a) Priming Coat:

25 pounds pure white lead
1 gallon pure raw linseed oil
½ gallon pure turpentine
¼ pint drier, free from rosin

(b) Body Coat:

25 pounds pure white lead
3⁄8 gallon pure raw linseed oil
3⁄8 gallon pure turpentine
¼ pint drier, free from rosin

(c) Finishing Coat:

25 pounds pure white lead
1 gallon pure raw linseed oil
¼ pint pure turpentine
¼ pint drier.

One must exercise his own discretion in using a larger or smaller quantity of oil according to whether the wood is oil absorbing, as white pine, poplar, and basswood, or less permeable, as yellow pine, cypress, spruce, and hemlock.

28. Formulas for Making Tinted Paint.—Any color or tint may be obtained by varying the addition of tinting colors. These tinting colors are called "colors in oil." The colors should be added to the white lead before the paint is thinned.

To twenty-five pounds of white lead ground in oil add colors in oil as follows:

Medium Blue Slate | 3½ oz. lamp black
Gray Blue | ¼ oz. lamp black
| 1 oz. Prussian blue
| ¼ oz. medium chrome green
Dark Drab | 5 lbs. French ochre
| ½ lb. lamp black
| ¼ lb. Venitian red
[Pg 27]
Dark Slate | 2 oz. lamp black
| 3 oz. medium chrome yellow
Dark Lilac | 1 oz. lamp black
| 5 oz. Venitian red
Lilac | ½ oz. lamp black
| 1½ oz. Venitian red
Forest Green | 1½ oz. lamp black
| 8 lbs. light green
| 5 oz. medium chrome yellow
Buff | 1½ lb. French ochre
| 3⁄8 oz. Venitian Red
Cream | 5 oz. French ochre
Sea Green | 3⁄8 oz. lamp black
| ½ oz. medium chrome green
| 1¼ oz. medium chrome yellow

Where tinting colors are used in sufficiently large quantities to alter the consistency of the paint, add one-half as much linseed oil and turpentine, by weight, as you add tinting material.

29. Enameling.—When using enamel as a finish for toys, care should be taken that the surface of the toy is in proper condition. To obtain good results proceed as follows: Give the wood a coat of shellac. Sand lightly and dust. The following coat should consist of part of white paint and one part of the enamel to be used. This coat should be slightly tinted with the finishing color, if the finishing coat is not white. Allow twenty-four hours for drying thoroly; then sand with No. OO sand paper. Next apply a coat of enamel of the color desired for the finished work. (Enamels may be tinted with colors ground in oil.)

Should the enamel not work freely, add a spoonful of benzine to a gallon of enamel. Turpentine may also be used as a thinner for enamel.

A better finish of enamel consists of two coats of paint before applying the enamel. This gives it a stronger body and of course makes it more durable.

Because of its durability and for sanitary reasons enamel is the most desirable finish for toys. Its glossy finish is attractive and very appealing to children.[Pg 28]

30. The Dipping Method.—When a considerable quantity of toys is to be finished, the problem to be faced will be the cost of application of the paint rather than the cost of the paint itself. The dipping process, (immersing the material to be covered) is found to be the most successful, especially in toy making, where so many small parts are used.

Many of the small pieces made can be subjected to the dipping process at quite a saving of time and labor, with probably better results than where the application of paint or stain is done with a brush.

The success of the dipping process depends on the arrangement adopted for holding the toys while the actual dipping is done and while they are drying. Here the exercise of a little ingenuity on the part of the students and teacher, will overcome most difficulties.

Supposing that a number of checkers, or handles, or small wheels are to be stained. A dipping frame as shown in Fig. 8 could very easily be prepared. You will notice the screen tray (which is removable), and the tin sheet which slopes towards the container. The small pieces to be stained can be handled in wire baskets with mesh just small enough so that the pieces will not fall thru.

The wire basket is then immersed in the container and worked up and down, so that the liquid will penetrate and touch all pieces. It is then pulled up and swung over the screen tray, where the contents of the wire basket is dumped. Here, the superfluous paint will drip off on the tin sheet, which, because of its slope, will cause the superfluous paint to flow back in to the container. Fig. 9 shows the dipping frame in use.

The screen tray can be removed and placed in a rack to allow for further drying. Several trays could then be made and a rack to hold them could very easily be constructed.

The paint used for dipping purposes must so be prepared that too much does not run off or too much stay on, for this is surely one way to spoil the work. It should be thinned to the right consistency and care should be taken that the thinners used are of the best quality.

Where larger pieces of work are to be dipped, wire attachments could be devised and each part hung separately over the dipping frame until ready to be placed in a rack. If the wire[Pg 29] attachment forms a hook on one end, it will be possible to hang up the toy until drained and dried. In removing the toy from the paint it should be drawn out very slowly so that the surface of the paint may be left as smooth as possible.

Where one desires line effects on toys, these may be lined in afterwards with a small size striping brush or sign painter's pencil.

Fig. 8. Dipping frame

[Pg 30]

Fig. 9. Using the dipping frame

[Pg 31]

31. Polishing by Tumbling.—-Excellent results in polishing large quantities of small pieces, may be obtained by tumbling. The material to be polished should be thoroly dry. The parts are then placed in a tumbler as shown in Fig. 10. Cut up paraffine wax into small pieces, using about one-fourth pound to each tumbler full of toys. Allow these to tumble several hours. This will distribute the wax evenly over the parts and produce a polished surface.

The tumbler as shown in Fig. 10 is turned by hand, altho it could very easily be placed in a lathe, where one is available.

Fig. 10. Tumbler for polishing small pieces

32. Care of Brushes.—A suitable place should be provided for brushes that are not in use. A tin-lined keeper is recommended. Brushes should be suspended so that their bristles will not touch the bottom of the keeper, and have the liquid in which they are kept come well up over the bristles, so that none of the paint or varnish may dry in the butt of the brush.

33. Paint Application by Means of Compressed Air.—In recent years, great advancement has been made in the application of paint by means of compressed air. The early use of pneumatic painting equipment was confined almost exclusively to the application of finishing materials such as japans, enamels, lacquers, varnishes, etc., on manufactured products. But in the past few years improvements have been made which eliminate all of the difficulties originally experienced and make possible the use of this method for interior and exterior painting, such as buildings, ships, etc.; and at present, a large portion of factory maintenance work is done in this manner. Excessive fumes have been eliminated and all materials can be applied without removing the volatile thinners, solvents, binders, etc., thru air reduction. This is brought about thru the use of low pressure and the perfection of ingenious patent nozzles and other improvements.[Pg 32]

[Pg 33]

34. Uses of Pneumatic Sprayers.—Pneumatic paint sprayers, or air brushes, are extensively used in the manufacture of toys, furniture, automobile bodies, sewing machines, telephones, electrical equipment; in fact, very nearly all manufactured products, as well as on ships, structural steel and iron work, bridges and buildings.

The speed of the air brush is very great compared with hand-brush work. Usually, an air-brush operator will accomplish as much in one hour as a hand or bristle-brush worker will in one day; and it is possible to obtain an even coating, free from sags, runs or brush-marks and better results are obtained than with the hand brush method. A film of paint can be applied in one operation equal to two hand-brush coats, as it is not necessary to reduce paints by thinning as much for air brush application, in a great many instances, as is the usual practice for hand-brushing. The air sprayer can also reach places inaccessible to the hand brush, and a perfect coat can be applied over rough, uneven surfaces, which could not be obtained by hand-brushing.

In considering pneumatic painting equipment, the most important thing to be kept in mind is the proper application of materials. This can be successfully accomplished only thru the use of compressed air at low pressures. By this is meant using only sufficient main-line air to lay the paint, enamel, varnish or whatever finish may be used, on the object. Excessive pressure results in fumes, waste of material and air reduction taking place. By air reduction is meant the removal of the more volatile solvents, thinners, binders, etc., thru evaporation, and the material thus loses its adherent and coherent properties.

Both types of air-brush equipment illustrated here require three cubic feet of air per minute to operate and the pressure necessary depends on the density, consistency or viscosity of the material used. For example, undercoaters, japans, etc.; require from twelve to fifteen pounds of pressure to apply perfectly; while enamels and varnishes take from eighteen to twenty-five pounds. Water stains require about five pounds of pressure.

35. Construction of Pneumatic Painting Outfit.—A pneumatic painting outfit for finishing work consists essentially of an air brush, either of the[Pg 34] attached-container type or the gun-type with separate paint tank, and a small compressor of sufficient capacity to operate the air brush, which can be belt-driven from shafting or direct connected. An exhaust hood with fan, for the removal of fumes, is advisable where the operation is reasonably continuous and especially where lacquers are used. The paint, ready for application, is poured into the tank; and the compressed air line leads to the tank with a branch line for air and paint from the tank to the nozzle of the gun type of machine; while only the air line is required with the attached-container type.

The air hose used is 5/16" in diameter while the paint or fluid hose is the same size. The paint hose is made of a special compound to resist the action of the thinners, solvents, etc., used in the paint; and it is important to have this correct, so that the lining will not disintegrate and clog the air brush or gun.

Fig. 11 shows a five-gallon container type. It will be noticed that the fluid connection is nearest the nozzle and that the air connection is at the bottom of the grip.

Fig. 11. A five-gallon air brush outfit

36. Special Attachments for Different Surfaces.—A cone nozzle is furnished for painting irregular surfaces and a fan nozzle for wide, flat work. Adjusting and locking the nozzle regulates the degree of atomization. The jets of the fan nozzle are depressed to prevent being knocked out of alignment. Final regulation of the flow of material is made on the back of the gun, independent of the pressure on the material container. A wide variety of adjustment is possible with this positive regulation.

The first pull on the trigger gives air only, which can be used for dusting ahead of the work; and as the trigger is released, the air valve closes last, which prevents clogging and dripping. When adjustments have been made the trigger action is the only moving part of the machine. Figs. 12 and 13 show the five-gallon container type in actual use.

Fig. 12. Using pneumatic paint sprayers
Fig. 13. A five-gallon outfit in actual use

37. Cleaning Pneumatic Machines.—It is not necessary to take the gun apart nor disconnect the hose to clean the machine. Thinner can be run thru the device without loss by placing a small can of reducer of the last material used in the machine, and forcing it thru in the usual manner.[Pg 35]

38. Directions for Cleaning Machine.—Close right-hand Air Valve and open release valve. Unscrew air nozzle a few turns. Obstruct outlet with thumb and pull trigger. Spraying pressure is thus forced thru gun and fluid hose and the material backed into the container. It is advisable frequently to run thinner thru the machine as follows: (1) Place small can of thin[Pg 36]ner in center of container directly beneath fluid tube. (2) Replace cover and tighten wing-nuts. (3) Close left-hand air valve and open right-hand air valve. Pressure on container will force thinner thru the machine and clean perfectly without loss. Do not use spraying pressure in cleaning. The thinner can be used again for either cleaning or thinning purposes.

Fig. 14. Attached container type of sprayer

39. Directions for Operating Pneumatic Equipment.—

1. Attach main-line air hose to air filter.

2. Attach fluid hose to connection marked "Fluid" on tank and to the front connection near air nozzle on hand-piece.[Pg 37]

3. Attach air hose to connection marked "Air" on cover and to the handle connection on hand-piece.

4. Thoroly mix and strain material so that it is entirely free from skins, lumps, and foreign materials.

5. Tighten wing-nuts until paint container is air-tight.

6. See that release valve is closed. Then open right-hand air valve, turn fluid-pressure regulator until gage shows 5 lbs. pressure in container. Pull trigger and use fluid regulator[Pg 38] on gun to control the flow. If material is heavy, increase pressure in container.

7. Open left-hand air valve and turn spraying pressure regulator until sufficient pressure (5 lbs. to 25 lbs.), is obtained to lay the material on.

8. Make final adjustment of the flow of material with fluid regulator on back of hand-piece and get proper spray by adjusting the air nozzle.

9. Spraying pressure and pressure in the container depends upon the density of the material used and the size of the surface to be coated. A little experimenting on the part of the operator will determine the best pressure to use. When the fan nozzle is used, 3 to 5 lbs. more pressure should be applied to the material container and from 5 to 8 lbs. more atomizing or spraying pressure used.

Fig. 14 shows a complete attached container which operates on identically the same principles as the type shown in Fig. 11. It consists of a 1½ pint container, reducing outfit, compressor, and air tank. The 1½ pint container as shown in Fig. 15 is supplied complete with two fluid tips, gasket, agitator tube, cup-holder, hose union, and six feet of air hose.

Fig. 15. A one and one-half pint container and parts
Fig. 16. Reducing outfit

The reducing outfit in Fig. 16 consists of a regulative valve, an air gage, and an air filter, complete with connections and fittings. This outfit is for the purpose of maintaining an even low spraying pressure.

Regulated pressure is applied to the air-tight material container, raising the coating[Pg 39] material to the nozzle where only sufficient main-line pressure is used to lay the coating on. The spraying pressure necessarily depends on the density, consistency and viscosity of the material used.

For fine finishing work, where the quantity of materials used each day is not great, or where the colors are changed frequently, the attached container type is recommended.

40. Preparing Colors.—The three primary colors are red, blue and yellow. With the three primary colors at hand, almost every variety of color desirable for ordinary use can be easily prepared. Fig. 17 shows a color chart.

Red mixed with yellow will result in orange.

Red mixed with blue will result in purple.

Yellow mixed with blue will result in green.

The colors obtained by mixing any two[Pg 40] primaries are called secondary colors. Therefor the secondary colors are orange, purple and green.

Orange mixed with purple will result in brown.

Orange mixed with green will result in olive.

Purple mixed with green will result in slate.

The colors obtained by mixing any two secondaries are called tertiary colors.

The tertiary colors are brown, olive and slate.

Of course different tones of each color can be made up by mixing unequal proportions.

[Pg 41]

Fig. 17. Chart showing proportions required for standard colors

[Pg 42]

## CHAPTER III

## Common Woods Used in Toy Making

41. Economy in Selecting Material.—Economic use of materials should be encouraged at all times. Toy making offers an excellent opportunity where economy may be taught in the most practical way.

Where toys are to be painted, more than one kind of wood may be used in the same toy and thereby using up small pieces of wood that would otherwise be called scrap. Yet, it is not advisable to sacrifice the strength and durability of the whole toy for the sake of using up a piece of scrap wood which weakens the particular part of the toy where it is used. For that, in the long run, is not economy.

42. Qualities of Different Woods Used.—The following are some of the common woods used in toy making.

Maple: hard, fine grained, compact, tough, used for wheels, axles, handles, dowel rods, etc.

Ash: white, strong, open grained, easily worked; used for bodies of coasters, wheels, axles, oars, etc.

Oak: hard, firm and compact, strong and durable, hard to work.

Birch: moderately hard and heavy, even grained; difficult to split, but easily worked.

Chestnut: resembles oak in appearance, is much softer, moderately hard, course grained, not strong, but durable.

Cypress: moderately hard, very fine and close grained, virtually indestructable; known as "the wood eternal".

Basswood: white, light, soft, tough, closed grained, easily worked, not strong, but durable; used for almost any part of a toy where much strength is not required.

White Pine: very light, soft, close and straight grained, inferior; easy to work.

Yellow Pine, yellowish, grain noticeable, harder than white pine, stronger.

Tulip (yellow poplar): light, soft, close and straight grained; tougher than many woods equally soft, compact, not very strong or durable, easily worked.

Spruce: straight growing, light, straight and even in grain, tough, elastic, easy to work.

[Pg 43]

## CHAPTER IV

## Use of Jigs and Fixtures

43. Value of Jigs and Fixtures.—The use of jigs, fixtures, and other labor-saving devices is an important factor in illustrating industrial and practical applications in the school shop. It is advisable to let each group of boys work out its own jig or fixture for the particular job they have on hand.

The three most common forms of jigs are cutting jigs, boring jigs, and assembling jigs. The important reasons for the use of such devices are: (1) They illustrate the speed of output in shop work. (2) They give the student a good idea of machine operation. (3) They help in making the parts interchangeable. (4) They offer an opportunity for getting first hand information on cutting edge tools and their proper uses. (5) They show the boy the value of the use of jigs in factory work.

The toys illustrated in this book have many simple operations, such as cutting stock to length, drilling holes, surfacing, etc., that can be easily done by the use of the proper fixtures.

For that reason toys are desirable projects to be made by the productive plan. Fig. 18 shows the use of a jig and the miter box.

44. Cutting Small Wheels.—A circle of the desired size wheel may be laid out on the wood with the aid of a compass, and cut in the outline with a coping saw or band saw. Of course, it would take quite a long time by this method to make the small wheels in large quantities and besides the result would not be as good as when the wheels are made by machine.

45. Turning Wheels.—Another way to produce wheels is to turn a cylinder to the required diameter, on the turning lathe. Then cut the cylinder on the circular saw into required thicknesses of wheels desired. This method is recommended for quick work.[Pg 44]

Fig. 18. Production of toys by use of jigs
Fig. 19. Wheel cutter in use

If it is desired to round the end of wheels the operation can be done by leaving the cylinder in the lathe and applying the broad side of the skew chisel as shown in Fig. 33. The wheels may then be polished with a cloth after they have been sanded and while rotating in the lathe as shown in Fig. 34. In sanding, use first a fairly course grade of sandpaper, No. 1 or 1½ and afterwards a fine grade, No. O or OO. Before applying the cloth the wood may be varnished lightly while the lathe is not running, taking care to wipe off all the surplus varnish. The varnish will assist in giving the surface a fine polish when the cloth is applied. For further explanations of the use of the turning lathe, see Sec. 55.

[Pg 45]

46. Use of Wheel Cutter.—Still another method of making small wheels is by use of the wheel cutter as shown in Fig. 19. This wheel cutter may be used in the ordinary bit brace. Good results may be obtained where the wheels are made out of thin, soft wood.

This wheel cutter is known on the market as a leather washer cutter. If one cannot be obtained it can easily be made in the school machine shop at a small cost. Fig. 20 shows a drawing of a wheel cutter.

You will notice that the blade can be adjusted to cut any diameter desired.

47. Use of Coping Saw.—Where a band saw is not included in the shop equipment, many articles such as animal forms and small wheels could very easily be cut out with a coping saw.

A saw board, as shown in Fig. 21 should be fastened to a table top with an iron clamp; or, a saw board made to fasten in a vise may also be used.

When cutting out the toy part, the coping saw should be held in a vertical position as shown in Fig. 22, and in an up-and-down motion,[Pg 46] with short fast strokes, following the outline carefully. Cut on the line. Do not press hard on the saw for the blade is very thin and can very easily be broken, but it should last a long time if used correctly.

Fig. 20. Details of a wheel cutter which may be made in school

[Pg 47]

Fig. 21. Clamping the saw board to the bench
Fig. 22. Correct method of holding coping saw
Fig. 23. Removing the saw-blade

48. Cutting Sharp Corners.—When cutting a sharp turn in the wood with the coping saw, care should be taken not to twist the saw blade out of shape. Upon reaching the sharp turn, continue the up-and-down motion, but without doing any cutting; turn the wood very slowly until you have made the complete turn, then continue with the sawing and follow the rest of[Pg 48] the outline carefully.

49. Removing the Saw-Blade from Frame.—To remove the saw-blade from the frame, place the head of the frame against the table top as shown in Fig. 23. Pressing down on the handle will release the saw-blade. When inserting the blade into the frame the same method may be followed, being careful that the teeth of the saw-blade point toward the handle of the frame. The blade may be put in the end or the side slots of the frame, using the side slots only when the end slots will not serve the purpose.

50. Making Heavy Wheels.—In turning heavier wheels that are to be used for coasters, kiddie cars, etc., the work is done with the head stock only, the wood being supported by the screw-center chuck or face plate.

In turning the wheel the first step is the scraping cut as shown in Fig. 24. This cut is properly made with the concave chisel held in such a position as to give a light scraping cut. Care should be exercised not to allow the chisel to extend too deeply, otherwise the material will chip with the grain.

After the desired circumference has been obtained the surface should be worked to the desired form as shown in Fig. 25. This is accomplished by using the lathe rest, set at right angles with the bed or parallel with the face plate. The illustration in Fig. 26 shows the use of the dividers in marking off the position of the various corrugations in the wheel that is being turned. The sanding should be done while[Pg 49] the wheel is in the lathe. Use first a fairly course grade of sand paper and afterwards a fine grade, No. O or OO.

51. Designs for Wheels.—Suggestions for wooden toy wheels are shown in Fig. 27. Those numbered 1, 2, 3, 4, 5, 6, and 7 are plain wooden wheels varying in design only. No. 8 and 9 are re-enforced with zinc and large iron washers. No. 10 shows a segment of an iron pipe fitted in the center of the wheel to prevent wearing away of material. No. 11 shows a spoke wheel. The spokes are made of dowel rods; these fitting into a hub that can easily be turned out on the lathe. No. 13 shows a wheel built in segments which is then cut out on the band saw to resemble a standard spoke wheel. The rim is 1/8" steel, fastened to spokes with very small rivets.

Fig. 24. Making heavy wheels. The scraping cut

52. Cutting Wheels on Band-Saw.—A circle of the required size wheel may be marked off on the wood with a compass, then cut in the outline on the band-saw. This method will leave square corners and will be more or less out of truth with the center of the wheel. To true up and smooth the outside of the wheel the lathe attachment as shown in Fig. 28 can be easily prepared. This attachment consists of a block A fastened to the lathe bed with a single bolt, and a stop B fastened to the upper face of the block A. The carriage C is a loose piece the same thickness as the stop B and is provided with a dowel rod to fit the central hole in the wheel. This dowel rod is so located that when the edge of the carriage C is tight against the edge of the stop D, the distance from the center of the dowel rod to the face of the abra[Pg 50]sive material on the disk, will be equal to the radius of the finished wheel.

The wood is cut out on the band saw a scant 1/16" over-size in diameter, and is then placed on the dowel rod in the carriage C which is held flat on block A while the edge of the blank is brought in contact with the grinding disc face by pushing the carriage forward with the left hand while the blank is slowly revolved with the right. This grinding is continued until the edges of stop B and carriage C will remain in contact during a complete revolution of the wheel blank. During this grinding process, the carriage should be moved back and forth from the edge to the center of the grinding disc so that the wear on the abrasive material may be equalized.

Fig. 25. Smoothing the side of wheels
Fig. 26. Using dividers to mark for cuts

A similar device used for chamfering the edges of the blanks is also shown in Fig. 28, as it looks when viewed from the front of the lathe. The preceding description will suffice for this as the same system of lettering has been used. It differs only in that block A is made to set at an angle of 45 degrees instead of being level.[Pg 51]

Fig. 27. Many ways of making wheels for toys

[Pg 52]

Fig. 28. Simple attachments which may be made for lathe

[Pg 53]

Grinding discs may be made either of metal or wood. Metal is preferable but a hardwood disc fastened to a metal face plate will answer very well. There are many methods of fastening the abrasing material to the disc but the most convenient way is by the use of stick belt dressing. The disc is coated with dressing by holding the stick against it as it revolves and the abrasive is applied before the dressing has set. A pair of dividers or trammels is used to cut the abrasive material to the same diameter as the disc and it should be warmed on the uncoated side before it is applied. It sticks tightly to the disc but is easily removed and replaced with fresh material in a few minutes.

53. Boring Holes in Wheels.—The center holes in wheels may be bored with bit and brace, but better results are obtained if the holes are bored in the lathe. A drill chuck fitted to the live spindle and a drilling pad for the tail stock spindle will be required to do this job efficiently. The tail stock is locked fast and the wheel to be drilled is placed against the drilling pad and fed up to the revolving bit by turning the tail spindle feed wheel. This method will produce a cleaner hole and one that is square with the wheel face.

[Pg 54]

## CHAPTER V

## Operation of Woodworking Machines

54. Importance of Machine Operations.—A fair understanding of what is the correct position to take at some of the principal machines such as the lathe, universal saw, jointer, and sander, is very important to the student in the wood-working department. Such knowledge is of special importance to the one engaged in toy making, where every knowledge of use of machines, is put to the test.

Fig. 29. The roughing cut
Fig. 30. The sizing cut

Sufficient examples are given to enable the student to arrive at a fair understanding of the correct postures.[Pg 55]

55. Operating the Lathe.—The lathe is perhaps one of the most important machines used in toy making. It lends itself to unlimited varieties of work and for that reason is really indispensible in the shop.

In Fig. 29 the student is preparing to take the roughing cut in turning a cylinder. This operation consists of removing the corners of the square piece and is done with the tool known as the gouge.

After the roughing cut has been taken, calipers set to the diameter desired will determine the depth of the next cut, sizing cut. The illustration in Fig. 30 shows the student performing this operation with the cut-off tool.

Fig. 31. The paring cut
Fig. 32. Using the cut-off tool

When the correct dimension has been found, the next step in the process of turning a cylinder is the paring cut or finishing cut, Fig. 31. This is done with the skew or bevel chisel. A very thin shaving is removed by this operation.[Pg 56]

The ends are then cut by using the cut-off tool as shown in Fig. 32. It is merely taking a slice off the end. If a very thin slice is to be removed, it is usually made by the long point of the skew chisel. If it is more than a quarter of an inch it should be sized and then removed by the skew.

If it is desired to round the end of a piece or to produce a convex surface the operation can be done by applying the broad side of the skew chisel, as in Fig. 33.

56. Face Plate Turning.—The preceding paragraphs describe the process of turning when the piece is supported between the live and the dead centers. The processes shown in Figs. 24, 25 and 26, illustrate the character of the work done with the head stock only when the piece is supported by the screw-center chuck or face plate.

Fig. 33. Making convex surfaces
Fig. 34. Polishing wood in lathe

The first step in face plate turning is the[Pg 57] scraping cut, Fig. 24. This cut is properly made with the concave chisel held in such a position as to give a light scraping cut. Care should be exercised not to allow the chisel to extend too deeply, otherwise the material will chip with the grain. After the desired circumference has been obtained the surface should be smoothed with the skew chisel.

Fig. 35. Cutting off stock
Fig. 36. Fluting on circular saw

Fig. 25 shows the student modeling a rosette, using the rest, set at right angles with the bed or parallel with the face plate. Prior to the modeling a shearing cut should be taken with[Pg 58] the skew chisel to face off the material to an even surface.

The illustration in Fig. 26 shows the use of the dividers. The student is marking off to a uniform scale the position of the various corrugations in the rosette he is turning.

57. The Universal Saw.—The operations that can be performed on the universal saw are so many that no attempt will be made to illustrate them all here. But enough are given to show the characteristic operations involved in cross-cutting, ripping, and dadoing,—the three basic uses of a circular saw.

Fig. 37. Cutting with special fence
Fig. 38. Grooving, or ripping special work

[Pg 59]

It is a more dangerous tool than the lathe and the guard should be kept over the saw at all times, except of course, in dadoing when it can not be used.

Figs. 35, 36, 37, 38, 39, illustrate the basic uses of a circular saw.

Fig. 39. Cutting segments
Fig. 40. Surfacing board on jointer

58. The Hand Jointer.—The great variety of work that can be done on a hand jointer depends very largely upon the knowledge and skill of the operator. It lends itself to so many operations, that the student gains much in knowledge and efficiency.[Pg 60]

Fig. 41. Cutting bevels on jointer
Fig. 42. Jointing the edge

The five operations shown in Figs. 40, 41, 42, 43 and 44, give a fair idea of the scope of work that is usually accomplished on a hand jointer and show something of the method by which the work should be done.

The jointer is another tool where the use of the guard should never be omitted.[Pg 61]

Fig. 43. Rabetting on the jointer
Fig. 44. Cutting miter joints

59. The Sander.—The sander is an interesting machine in the school shop for on it considerable "forming" can be done as with the lathe, altho its prime use is to make smooth or polish.

In Fig. 45 the boy at the left is forming a mitre while the one on the right is smoothing surface.

[Pg 62]

Fig. 45. The machine sander in operation

[Pg 63]

# PART II.

# Drawings For Toys

[Pg 64]

PLATE 1

[Pg 65]

PLATE 2

[Pg 66]

PLATE 3

[Pg 67]

PLATE 4

[Pg 68]

PLATE 5

[Pg 69]

PLATE 6

[Pg 70]

PLATE 7

[Pg 71]

PLATE 8

[Pg 72]

PLATE 9

[Pg 73]

PLATE 10

[Pg 74]

PLATE 11

[Pg 75]

PLATE 12

[Pg 76]

PLATE 13

[Pg 77]

PLATE 14

[Pg 78]

PLATE 15

[Pg 79]

PLATE 16

[Pg 80]

PLATE 17

[Pg 81]

PLATE 18

[Pg 82]

PLATE 19

[Pg 83]

PLATE 20

[Pg 84]

PLATE 21

[Pg 85]

PLATE 22

[Pg 86]

PLATE 23

[Pg 87]

PLATE 24

[Pg 88]

PLATE 25

[Pg 89]

PLATE 26

[Pg 90]

PLATE 27

[Pg 91]

PLATE 28

[Pg 92]

PLATE 29

[Pg 93]

PLATE 30

[Pg 94]

PLATE 31

[Pg 95]

PLATE 32

[Pg 96]

PLATE 33

[Pg 97]

PLATE 34

[Pg 98]

PLATE 35

[Pg 99]

PLATE 36

[Pg 100]

PLATE 37

[Pg 101]

PLATE 38

[Pg 102]

PLATE 39

[Pg 103]

PLATE 40

[Pg 104]

PLATE 41

[Pg 105]

PLATE 42

[Pg 106]

PLATE 43

[Pg 107]

PLATE 44

[Pg 108]

PLATE 45

[Pg 109]

PLATE 46

[Pg 110]

PLATE 47

[Pg 111]

PLATE 48

[Pg 112]

PLATE 49

[Pg 113]

PLATE 50

[Pg 114]

PLATE 51

[Pg 115]

PLATE 52

[Pg 116]

PLATE 53

[Pg 117]

PLATE 54

[Pg 118]

## INDEX

| PAGE
A
Auto kar, Plate 41 | 104
Auto racer, Plate 9 | 72
Auto Roadster, Plate 8 | 71
B
Bats, base ball, Plate 54 | 117
Bazaars, toy sales, etc. | 19
Bed, doll's, Plates 22, 23 | 85, 86
Boring holes in wheels | 53
Brushes, care of | 31
Buffet, Plate 14 | 77
C
Car, baby's, Plate 36 | 99
Car, passenger, Plate 10 | 73
Cars, auto, motor, choo-choo, Plates 41, 42 | 104, 105
Cart, baby's, Plate 3 | 66
Cart, hay, Plate 4 | 67
Carriage, dolls, Plate 17 | 80
Chair & rocker, Plate 13 | 76
Chair, baby's, Plate 47 | 110
Checker board, Plate 45 | 108
Check, credit, Fig. 7 | 20
Coasters, Plates 26, 37, 39 | 89, 101, 103
Coloring toys | 21
Sanitation emphasized | 21
Preparation of surfaces | 21
Application of water colors | 21
Analine water stains | 22
Formulas for analine water stains | 22
Oil stains | 23
Shellacking | 23
Varnishing | 23
Points on varnishing | 24
Color varnish | 24
Use of paint | 24
Dipping method | 28, 30
Polishing by tumbling | 31
Paint application by compressed air | 31
Colors, preparing | 39
Color chart, Fig. 17 | 41
Contents, Table of | 5
Coping saw, use of | 45
Correlation | 7
Costumer, child's, Plate 46 | 109
D
Doll's house, Plates 50, 51, 52 | 113, 114, 115
Dipping frame | 29
Drawings for toys | 63
Dumb bell, Plate 53 | 116
E
Enameling | 27
F
Foremen, shop | 11
Fox & geese game, Plate 1 | 64
Furniture, doll[Pg 119] | 75, 76, 77
G
Game board, "Bean Bag," Plate 19 | 82
Game board, "Fox & Geese," Plate 1 | 64
Grading students | 17
H
Horse head, Plate 5 | 68
Horse on wheels, Plate 6 | 69
House, doll's, Plates 50, 51, 52 | 113, 114, 115
I
Indian club, Plate 53 | 116
J
Jigs & fixtures | 43
Jointer, hand | 59
K
Kiddie kars, Plates 27, 28, 29 | 90, 91, 92
L
Lathe, operating the | 54, 55, 56, 57
M
Machines, operating of woodworking | 54
N
Noah's ark, Plate 18 | 81
O
Organization, plan for shop | 11
P
Paint, use of | 24
Ingredients of | 24
Application | 25
Preparation of surface | 25
Tinting materials | 25
Mixing | 25
Formulas | 26
Formulas for tinted paint | 26
Enameling | 27
Plan for shop organization | 11
Grouping students | 11
Time clerk | 13
Tool-room clerk | 13
Recording attendance | 14
Time-card rack | 14
Time cards | 15
Grading students | 17
Accomplishment sheet | 18
Preparation for shop work | 19
Pneumatic equipment | 36
Preface | 3
Productive work | 11
R
Ring toss, Plate 2 | 65
Rocking chair, Plate 13 | 76
Rocker, duck, Plate 35 | 98
Rocker, ducky loo, Plate 34 | 97
Rock-a-doodle, Plate 31 | 94
S
Sand box, Plates 48, 49 | 111, 112
Sander | 60, 62
Saw, universal | 58
Scooter, Plate 25 | 88
Sleds, Plates 32, 33 | 95, 96
Sprayer, pneumatic air[Pg 120] | 31, 33, 34
Sprayer, directions for operating | 36
Speedster, duplex, Plate 30 | 93
Stain, oil | 23
Stain, analine water | 22
Stilts, adjustable, Plate 24 | 87
Suggestions to teachers | 7
Swing, child's, Plates 20, 21 | 83, 84
T
Table for doll house, Plate 12 | 75
Teeter-totter, Plate 43 | 106
Teeter-rocker, Plate 44 | 107
Time clerk | 13
Time cards | 15
Tool-room clerk | 13
Toy sales | 19
Trailer, kido-kar, Plate 7 | 70
Tumbler, drawing of | 32
Tumbling, polishing by | 31, 32
V
Varnishing | 23
Varnish, colored | 24
Varnishing, points on | 24
W
Wagon, milk, Plate 11 | 74
Water colors | 21
Wax polishing | 31
Wheel-barrow, toy, Plate 15 | 78
Wheel-barrow, horse design, Plate 16 | 79
Wheel cutter | 45, 46
Wheels, cutting small | 43
Wheels, designs, Fig. 27 | 49, 51
Wheels, turning | 43
Woods used in toy making | 42

***END OF THE PROJECT GUTENBERG EBOOK ADVANCED TOY MAKING FOR SCHOOLS***

******* This file should be named 36815-h.txt or 36815-h.zip *******

This and all associated files of various formats will be found in:
http://www.gutenberg.org/3/6/8/1/36815

Updated editions will replace the previous one--the old editions will be renamed.

Creating the works from public domain print editions means that no one owns a United States copyright in these works, so the Foundation (and you!) can copy and distribute it in the United States without permission and without paying copyright royalties. Special rules, set forth in the General Terms of Use part of this license, apply to copying and distributing Project Gutenberg-tm electronic works to protect the PROJECT GUTENBERG-tm concept and trademark. Project Gutenberg is a registered trademark, and may not be used if you charge for the eBooks, unless you receive specific permission. If you do not charge anything for copies of this eBook, complying with the rules is very easy. You may use this eBook for nearly any purpose such as creation of derivative works, reports, performances and research. They may be modified and printed and given away--you may do practically ANYTHING with public domain eBooks. Redistribution is subject to the trademark license, especially commercial redistribution.

    *** START: FULL LICENSE ***

    THE FULL PROJECT GUTENBERG LICENSE
    PLEASE READ THIS BEFORE YOU DISTRIBUTE OR USE THIS WORK

    To protect the Project Gutenberg-tm mission of promoting the free
    distribution of electronic works, by using or distributing this work
    (or any other work associated in any way with the phrase "Project
    Gutenberg"), you agree to comply with all the terms of the Full Project
    Gutenberg-tm License (available with this file or online at
    http://www.gutenberg.org/license).

    Section 1.  General Terms of Use and Redistributing Project Gutenberg-tm
    electronic works

    1.A.  By reading or using any part of this Project Gutenberg-tm
    electronic work, you indicate that you have read, understand, agree to
    and accept all the terms of this license and intellectual property
    (trademark/copyright) agreement.  If you do not agree to abide by all
    the terms of this agreement, you must cease using and return or destroy
    all copies of Project Gutenberg-tm electronic works in your possession.
    If you paid a fee for obtaining a copy of or access to a Project
    Gutenberg-tm electronic work and you do not agree to be bound by the
    terms of this agreement, you may obtain a refund from the person or
    entity to whom you paid the fee as set forth in paragraph 1.E.8.

    1.B.  "Project Gutenberg" is a registered trademark.  It may only be
    used on or associated in any way with an electronic work by people who
    agree to be bound by the terms of this agreement.  There are a few
    things that you can do with most Project Gutenberg-tm electronic works
    even without complying with the full terms of this agreement.  See
    paragraph 1.C below.  There are a lot of things you can do with Project
    Gutenberg-tm electronic works if you follow the terms of this agreement
    and help preserve free future access to Project Gutenberg-tm electronic
    works.  See paragraph 1.E below.

    1.C.  The Project Gutenberg Literary Archive Foundation ("the Foundation"
    or PGLAF), owns a compilation copyright in the collection of Project
    Gutenberg-tm electronic works.  Nearly all the individual works in the
    collection are in the public domain in the United States.  If an
    individual work is in the public domain in the United States and you are
    located in the United States, we do not claim a right to prevent you from
    copying, distributing, performing, displaying or creating derivative
    works based on the work as long as all references to Project Gutenberg
    are removed.  Of course, we hope that you will support the Project
    Gutenberg-tm mission of promoting free access to electronic works by
    freely sharing Project Gutenberg-tm works in compliance with the terms of
    this agreement for keeping the Project Gutenberg-tm name associated with
    the work.  You can easily comply with the terms of this agreement by
    keeping this work in the same format with its attached full Project
    Gutenberg-tm License when you share it without charge with others.

    1.D.  The copyright laws of the place where you are located also govern
    what you can do with this work.  Copyright laws in most countries are in
    a constant state of change.  If you are outside the United States, check
    the laws of your country in addition to the terms of this agreement
    before downloading, copying, displaying, performing, distributing or
    creating derivative works based on this work or any other Project
    Gutenberg-tm work.  The Foundation makes no representations concerning
    the copyright status of any work in any country outside the United
    States.

    1.E.  Unless you have removed all references to Project Gutenberg:

    1.E.1.  The following sentence, with active links to, or other immediate
    access to, the full Project Gutenberg-tm License must appear prominently
    whenever any copy of a Project Gutenberg-tm work (any work on which the
    phrase "Project Gutenberg" appears, or with which the phrase "Project
    Gutenberg" is associated) is accessed, displayed, performed, viewed,
    copied or distributed:

    This eBook is for the use of anyone anywhere at no cost and with
    almost no restrictions whatsoever.  You may copy it, give it away or
    re-use it under the terms of the Project Gutenberg License included
    with this eBook or online at www.gutenberg.org

    1.E.2.  If an individual Project Gutenberg-tm electronic work is derived
    from the public domain (does not contain a notice indicating that it is
    posted with permission of the copyright holder), the work can be copied
    and distributed to anyone in the United States without paying any fees
    or charges.  If you are redistributing or providing access to a work
    with the phrase "Project Gutenberg" associated with or appearing on the
    work, you must comply either with the requirements of paragraphs 1.E.1
    through 1.E.7 or obtain permission for the use of the work and the
    Project Gutenberg-tm trademark as set forth in paragraphs 1.E.8 or
    1.E.9.

    1.E.3.  If an individual Project Gutenberg-tm electronic work is posted
    with the permission of the copyright holder, your use and distribution
    must comply with both paragraphs 1.E.1 through 1.E.7 and any additional
    terms imposed by the copyright holder.  Additional terms will be linked
    to the Project Gutenberg-tm License for all works posted with the
    permission of the copyright holder found at the beginning of this work.

    1.E.4.  Do not unlink or detach or remove the full Project Gutenberg-tm
    License terms from this work, or any files containing a part of this
    work or any other work associated with Project Gutenberg-tm.

    1.E.5.  Do not copy, display, perform, distribute or redistribute this
    electronic work, or any part of this electronic work, without
    prominently displaying the sentence set forth in paragraph 1.E.1 with
    active links or immediate access to the full terms of the Project
    Gutenberg-tm License.

    1.E.6.  You may convert to and distribute this work in any binary,
    compressed, marked up, nonproprietary or proprietary form, including any
    word processing or hypertext form.  However, if you provide access to or
    distribute copies of a Project Gutenberg-tm work in a format other than
    "Plain Vanilla ASCII" or other format used in the official version
    posted on the official Project Gutenberg-tm web site (www.gutenberg.org),
    you must, at no additional cost, fee or expense to the user, provide a
    copy, a means of exporting a copy, or a means of obtaining a copy upon
    request, of the work in its original "Plain Vanilla ASCII" or other
    form.  Any alternate format must include the full Project Gutenberg-tm
    License as specified in paragraph 1.E.1.

    1.E.7.  Do not charge a fee for access to, viewing, displaying,
    performing, copying or distributing any Project Gutenberg-tm works
    unless you comply with paragraph 1.E.8 or 1.E.9.

    1.E.8.  You may charge a reasonable fee for copies of or providing
    access to or distributing Project Gutenberg-tm electronic works provided
    that

    - You pay a royalty fee of 20% of the gross profits you derive from
         the use of Project Gutenberg-tm works calculated using the method
         you already use to calculate your applicable taxes.  The fee is
         owed to the owner of the Project Gutenberg-tm trademark, but he
         has agreed to donate royalties under this paragraph to the
         Project Gutenberg Literary Archive Foundation.  Royalty payments
         must be paid within 60 days following each date on which you
         prepare (or are legally required to prepare) your periodic tax
         returns.  Royalty payments should be clearly marked as such and
         sent to the Project Gutenberg Literary Archive Foundation at the
         address specified in Section 4, "Information about donations to
         the Project Gutenberg Literary Archive Foundation."

    - You provide a full refund of any money paid by a user who notifies
         you in writing (or by e-mail) within 30 days of receipt that s/he
         does not agree to the terms of the full Project Gutenberg-tm
         License.  You must require such a user to return or
         destroy all copies of the works possessed in a physical medium
         and discontinue all use of and all access to other copies of
         Project Gutenberg-tm works.

    - You provide, in accordance with paragraph 1.F.3, a full refund of any
         money paid for a work or a replacement copy, if a defect in the
         electronic work is discovered and reported to you within 90 days
         of receipt of the work.

    - You comply with all other terms of this agreement for free
         distribution of Project Gutenberg-tm works.

    1.E.9.  If you wish to charge a fee or distribute a Project Gutenberg-tm
    electronic work or group of works on different terms than are set
    forth in this agreement, you must obtain permission in writing from
    both the Project Gutenberg Literary Archive Foundation and Michael
    Hart, the owner of the Project Gutenberg-tm trademark.  Contact the
    Foundation as set forth in Section 3 below.

    1.F.

    1.F.1.  Project Gutenberg volunteers and employees expend considerable
    effort to identify, do copyright research on, transcribe and proofread
    public domain works in creating the Project Gutenberg-tm
    collection.  Despite these efforts, Project Gutenberg-tm electronic
    works, and the medium on which they may be stored, may contain
    "Defects," such as, but not limited to, incomplete, inaccurate or
    corrupt data, transcription errors, a copyright or other intellectual
    property infringement, a defective or damaged disk or other medium, a
    computer virus, or computer codes that damage or cannot be read by
    your equipment.

    1.F.2.  LIMITED WARRANTY, DISCLAIMER OF DAMAGES - Except for the "Right
    of Replacement or Refund" described in paragraph 1.F.3, the Project
    Gutenberg Literary Archive Foundation, the owner of the Project
    Gutenberg-tm trademark, and any other party distributing a Project
    Gutenberg-tm electronic work under this agreement, disclaim all
    liability to you for damages, costs and expenses, including legal
    fees.  YOU AGREE THAT YOU HAVE NO REMEDIES FOR NEGLIGENCE, STRICT
    LIABILITY, BREACH OF WARRANTY OR BREACH OF CONTRACT EXCEPT THOSE
    PROVIDED IN PARAGRAPH 1.F.3.  YOU AGREE THAT THE FOUNDATION, THE
    TRADEMARK OWNER, AND ANY DISTRIBUTOR UNDER THIS AGREEMENT WILL NOT BE
    LIABLE TO YOU FOR ACTUAL, DIRECT, INDIRECT, CONSEQUENTIAL, PUNITIVE OR
    INCIDENTAL DAMAGES EVEN IF YOU GIVE NOTICE OF THE POSSIBILITY OF SUCH
    DAMAGE.

    1.F.3.  LIMITED RIGHT OF REPLACEMENT OR REFUND - If you discover a
    defect in this electronic work within 90 days of receiving it, you can
    receive a refund of the money (if any) you paid for it by sending a
    written explanation to the person you received the work from.  If you
    received the work on a physical medium, you must return the medium with
    your written explanation.  The person or entity that provided you with
    the defective work may elect to provide a replacement copy in lieu of a
    refund.  If you received the work electronically, the person or entity
    providing it to you may choose to give you a second opportunity to
    receive the work electronically in lieu of a refund.  If the second copy
    is also defective, you may demand a refund in writing without further
    opportunities to fix the problem.

    1.F.4.  Except for the limited right of replacement or refund set forth
    in paragraph 1.F.3, this work is provided to you 'AS-IS,' WITH NO OTHER
    WARRANTIES OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO
    WARRANTIES OF MERCHANTIBILITY OR FITNESS FOR ANY PURPOSE.

    1.F.5.  Some states do not allow disclaimers of certain implied
    warranties or the exclusion or limitation of certain types of damages.
    If any disclaimer or limitation set forth in this agreement violates the
    law of the state applicable to this agreement, the agreement shall be
    interpreted to make the maximum disclaimer or limitation permitted by
    the applicable state law.  The invalidity or unenforceability of any
    provision of this agreement shall not void the remaining provisions.

    1.F.6.  INDEMNITY - You agree to indemnify and hold the Foundation, the
    trademark owner, any agent or employee of the Foundation, anyone
    providing copies of Project Gutenberg-tm electronic works in accordance
    with this agreement, and any volunteers associated with the production,
    promotion and distribution of Project Gutenberg-tm electronic works,
    harmless from all liability, costs and expenses, including legal fees,
    that arise directly or indirectly from any of the following which you do
    or cause to occur: (a) distribution of this or any Project Gutenberg-tm
    work, (b) alteration, modification, or additions or deletions to any
    Project Gutenberg-tm work, and (c) any Defect you cause.

    Section  2.  Information about the Mission of Project Gutenberg-tm

    Project Gutenberg-tm is synonymous with the free distribution of
    electronic works in formats readable by the widest variety of computers
    including obsolete, old, middle-aged and new computers.  It exists
    because of the efforts of hundreds of volunteers and donations from
    people in all walks of life.

    Volunteers and financial support to provide volunteers with the
    assistance they need are critical to reaching Project Gutenberg-tm's
    goals and ensuring that the Project Gutenberg-tm collection will
    remain freely available for generations to come.  In 2001, the Project
    Gutenberg Literary Archive Foundation was created to provide a secure
    and permanent future for Project Gutenberg-tm and future generations.
    To learn more about the Project Gutenberg Literary Archive Foundation
    and how your efforts and donations can help, see Sections 3 and 4
    and the Foundation web page at http://www.gutenberg.org/fundraising/pglaf.

    Section 3.  Information about the Project Gutenberg Literary Archive
    Foundation

    The Project Gutenberg Literary Archive Foundation is a non profit
    501(c)(3) educational corporation organized under the laws of the
    state of Mississippi and granted tax exempt status by the Internal
    Revenue Service.  The Foundation's EIN or federal tax identification
    number is 64-6221541.  Contributions to the Project Gutenberg
    Literary Archive Foundation are tax deductible to the full extent
    permitted by U.S. federal laws and your state's laws.

    The Foundation's principal office is located at 4557 Melan Dr. S.
    Fairbanks, AK, 99712., but its volunteers and employees are scattered
    throughout numerous locations.  Its business office is located at
    809 North 1500 West, Salt Lake City, UT 84116, (801) 596-1887, email
    business@pglaf.org.  Email contact links and up to date contact
    information can be found at the Foundation's web site and official
    page at http://www.gutenberg.org/about/contact

    For additional contact information:
         Dr. Gregory B. Newby
         Chief Executive and Director
         gbnewby@pglaf.org

    Section 4.  Information about Donations to the Project Gutenberg
    Literary Archive Foundation

    Project Gutenberg-tm depends upon and cannot survive without wide
    spread public support and donations to carry out its mission of
    increasing the number of public domain and licensed works that can be
    freely distributed in machine readable form accessible by the widest
    array of equipment including outdated equipment.  Many small donations
    ($1 to $5,000) are particularly important to maintaining tax exempt
    status with the IRS.

    The Foundation is committed to complying with the laws regulating
    charities and charitable donations in all 50 states of the United
    States.  Compliance requirements are not uniform and it takes a
    considerable effort, much paperwork and many fees to meet and keep up
    with these requirements.  We do not solicit donations in locations
    where we have not received written confirmation of compliance.  To
    SEND DONATIONS or determine the status of compliance for any
    particular state visit http://www.gutenberg.org/fundraising/pglaf

    While we cannot and do not solicit contributions from states where we
    have not met the solicitation requirements, we know of no prohibition
    against accepting unsolicited donations from donors in such states who
    approach us with offers to donate.

    International donations are gratefully accepted, but we cannot make
    any statements concerning tax treatment of donations received from
    outside the United States.  U.S. laws alone swamp our small staff.

    Please check the Project Gutenberg Web pages for current donation
    methods and addresses.  Donations are accepted in a number of other
    ways including checks, online payments and credit card donations.
    To donate, please visit: http://www.gutenberg.org/fundraising/donate

    Section 5.  General Information About Project Gutenberg-tm electronic
    works.

    Professor Michael S. Hart is the originator of the Project Gutenberg-tm
    concept of a library of electronic works that could be freely shared
    with anyone.  For thirty years, he produced and distributed Project
    Gutenberg-tm eBooks with only a loose network of volunteer support.

    Project Gutenberg-tm eBooks are often created from several printed
    editions, all of which are confirmed as Public Domain in the U.S.
    unless a copyright notice is included.  Thus, we do not necessarily
    keep eBooks in compliance with any particular paper edition.

    Each eBook is in a subdirectory of the same number as the eBook's
    eBook number, often in several formats including plain vanilla ASCII,
    compressed (zipped), HTML and others.

    Corrected EDITIONS of our eBooks replace the old file and take over
    the old filename and etext number.  The replaced older file is renamed.
    VERSIONS based on separate sources are treated as new eBooks receiving
    new filenames and etext numbers.

    Most people start at our Web site which has the main PG search facility:

    http://www.gutenberg.org

    This Web site includes information about Project Gutenberg-tm,
    including how to make donations to the Project Gutenberg Literary
    Archive Foundation, how to help produce our new eBooks, and how to
    subscribe to our email newsletter to hear about new eBooks.

    EBooks posted prior to November 2003, with eBook numbers BELOW #10000,
    are filed in directories based on their release date.  If you want to
    download any of these eBooks directly, rather than using the regular
    search system you may utilize the following addresses and just
    download by the etext year.

    http://www.gutenberg.org/dirs/etext06/

        (Or /etext 05, 04, 03, 02, 01, 00, 99,
         98, 97, 96, 95, 94, 93, 92, 92, 91 or 90)

    EBooks posted since November 2003, with etext numbers OVER #10000, are
    filed in a different way.  The year of a release date is no longer part
    of the directory path.  The path is based on the etext number (which is
    identical to the filename).  The path to the file is made up of single
    digits corresponding to all but the last digit in the filename.  For
    example an eBook of filename 10234 would be found at:

    http://www.gutenberg.org/dirs/1/0/2/3/10234

    or filename 24689 would be found at:
    http://www.gutenberg.org/dirs/2/4/6/8/24689

    An alternative method of locating eBooks:
    http://www.gutenberg.org/dirs/GUTINDEX.ALL

    *** END: FULL LICENSE ***